# Purpose of this Equipment: To weigh boxes during the receiving process and in-house inventories to ensure accurate weight

1. **Federal Supply Class:** 6670
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Scale: 16 inches long / wide (+/- 3”), 25 inches deep (+/- 3”), 30 inches high. Dimensional sizes, such as length, width, and height are not critical to this equipment so long as this equipment is a floor model, and serves as a general guide to keep this equipment sized for available space.
      2. Movable Cart: 36 inches deep / wide (+/-3”), 15 inches high (+/-2”) (platform upon which the scales sits).
   2. **Salient Characteristics that shall be provided:**
      1. Scale:
         1. Stainless steel
         2. 300 pound weighing capacity
         3. Leveling legs
         4. Dual powered, battery and AC adaptor operable
      2. Display:
         1. Liquid Crystal Display (LCD) or Light Emitting Diode (LED)
         2. Weight displayed in 0.1 pound increments
         3. Tare indicator (shows weight of empty container)
      3. Movable Cart:
         1. Stainless steel
         2. Swivel casters, 2 locking

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N/A

# Color Requirement(s): N/A

1. **Electrical Requirements:**

# Standard U.S.A. electrical specifications: 120 volts, 60 Hertz, 1 phase.

# \_\_\_\_\_ Pacific Theater stores 120 V / 50 HZ / 1 PH (Applies to these stores only: Atsugi, Misawa, Sagami, Sagamihara, Yokosuka, Yokota, Camp Zama, and Kanto Plains CDC. All other stores are standard U.S.A. 60 cycle voltages.)

# NOTE: the operating range for 120 volts is 110 to 120 volts.

# Standard Contractor Requirements:

* + 1. Must be shipped ready to assemble, plug in, and use.
    2. This equipment requires disposal: place in a specified area.
  1. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  2. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****