1. **Purpose of this Equipment:** To load and move palletized product around the stockroom and store.
2. **Federal Supply Class:** 3920
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. Not to exceed 63 inches long, 27 inches wide, 49 inches high.
	2. **Salient Characteristics that shall be provided:**
		1. Manually operated
		2. Single Pallet
		3. Hydraulic lift mechanism
		4. 48 inch fork length
		5. Polyurethane wheels
		6. Steering wheels to be a minimum diameter of 7 inches
		7. Minimum 5000 pound load capacity

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements**: N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****