1. **Purpose of this Equipment:** To load and move palletized product around the stockroom and store.
2. **Federal Supply Class:** 3920
3. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Not to exceed 63 inches long, 27 inches wide, 49 inches high.
   2. **Salient Characteristics that shall be provided:**
      1. Manually operated
      2. Single Pallet
      3. Hydraulic lift mechanism
      4. 48 inch fork length
      5. Polyurethane wheels
      6. Steering wheels to be a minimum diameter of 7 inches
      7. Minimum 5000 pound load capacity

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements**: N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****