**STORE NAME: DODAAC:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

(Store name and DODAAC number to be completed when submitted.)

**STORE REQUIREMENT: *\_\_\_\_\_*** (ea)

**UNIT OF PACK (UPK):** 1 (one) each

1. **Purpose of Equipment:** To allow for hands free washing and sanitizing of the hands for employees processing food items.
2. **Generalized Operating Specifications:**
	1. Dimensions:
		1. Minimum 18 inches wide, 16 inches deep, 42 inches high (sink surface 34 inches high).
	2. Construction:
		1. Commercial off the shelf (COTS) standard unit, no unique DeCA requirements.
	3. Operating Characteristics that shall be provided:

# Expected life span of this equipment is required to be 12 years or more with basic maintenance.

* + 1. Hands free electronic faucet utilizing an infrared / motion sensing technology to sense the user’s presence to turn water on.
		2. Water temperature set by pre-set mixing valves.
		3. Standard gooseneck style faucet.
		4. Chrome plated brass fittings.
		5. Sink / countertop edge with no-drip offset.
		6. Satin finish surfaces.
		7. Heavy gauge 304 stainless steel.
		8. Pedestal skirt.
		9. Soap dispenser.
		10. Equipment is a pedestal style floor model.
	1. Networking / Communications that shall be provided: N / A
1. **Operating Options:** N / A
2. **Electrical Requirements:**

# Standard U.S.A electrical specifications: 120 volts, 60 Hertz, 1 phase, with an average amperage draw of 4 amps.

# \_\_\_\_\_ Pacific overseas store 220 V / 50 HZ / 1 PH

# \_\_\_\_\_ Europe overseas store 110 V / 50 HZ / 1 PH

1. **Color Requirements:** N / A
2. **Maintenance Sustainability Requirements:** Continued parts support for equipment is required for the projected total life cycle of the equipment plus 5 years.
3. **Industry Standards and Contractor Requirements:**
	1. Industry Standards: National Sanitation Foundation (NSF) certification, or equivalent.
	2. Contractor Requirements:
		1. Must be shipped ready to assemble, mount, make utility connections, and use.
		2. Operational testing.
		3. No additional work shall be required on the part of the government.

# Special / Specific Equipment Safety Requirements: N / A

1. **Information To Be Provided By The Contractor To The Commissary At Time of Delivery:**
	1. Commercial Warranty and Point of Contact for Warranty Service.
	2. Installation and Operating Instructions.
	3. Parts List.

# Federal Supply Class: 4510

1. **Special Considerations For Installation/De-installation Of Equipment: (NOTICE/WARNING)**
	1. **Contractor**: N / A
	2. **Store**: Contact DeCA facility engineers.
2. **Basis of Allocation:** As required.
3. **Recommended Source(s) or equal:**
	1. Advance Tabco, model # 7-PS-91
4. **Store Request for Specific Model to Match Existing Equipment:** N / A
5. **Store Maintenance Requirements:** The purpose of maintenance planning is to sustain equipment operations post purchase, to identify maintenance requirements, to reduce maintenance costs, and to extend the life cycle of the equipment.
	1. **Within Warranty Period:**
		1. Consult manufacturer’s warranty documentation and contact instructions.
	2. **After Warranty Period:**
		1. Self-repair or replace the unit as required.
		2. Follow the Facility Maintenance Contract procedures for service.