1. **Purpose of this Equipment:** To trim, cut and de-bone meat items for special orders and for special wrapping.
2. **Federal Supply Class:** 7320
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. 4TMP-4: 48 inches long / wide, 30 inches deep, 34 inches high. Dimensional sizes, such as length, width, and height should not vary more than a plus or minus 2 inches.
		2. 4TMP-6: 72 inches long / wide, 30 inches deep, 34 inches high. Dimensional sizes, such as length, width, and height should not vary more than a plus or minus 2 inches.
	2. **Salient Characteristics that shall be provided:**
		1. Table and optional understructure shall be 16 gauge, 300 series stainless steel
		2. Legs to be stainless steel and a minimum of 1 5/8 inches diameter, with adjustable bullet feet
		3. Cutting surface is minimum 0.60 inch thick polyethylene
		4. Reversible polyethylene boards to come in two or three sections, depending on the length of the table
		5. Polyethylene boards to be dishwasher-safe and able to be steam cleaned at temperatures up to 180 degrees Fahrenheit without damaging the finish
		6. Tabletop is an open frame with the polyethylene boards resting on hat channels
		7. Corner tabs or similar means to hold polyethylene boards securely in place
		8. Shipped fully assembled
		9. Optional pan / boat racks, either wall or table mount
		10. Optional back splash

# Industry Standards / Requirement(s):

* + 1. National Sanitation Foundation (NSF) certification, or equivalent.
		2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped assembled and ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

 ****

* 1. 4 TMP-4 (4 foot)

 \_\_\_\_\_\_\_ Optional under-shelf.

 \_\_\_\_\_\_\_ Optional boat rack (wall mount style)

 \_\_\_\_\_\_\_ Optional boat rack (table mount style)

 \_\_\_\_\_\_\_ Optional backsplash

* 1. 4TMP-6 (6 foot)

 \_\_\_\_\_\_\_ Optional under-shelf.

 \_\_\_\_\_\_\_ Optional boat rack (wall mount style)

 \_\_\_\_\_\_\_ Optional boat rack (table mount style)

 \_\_\_\_\_\_\_ Optional backsplash