# Purpose of this Equipment: To provide a safe and sanitary area for parents to attend to the needs of their babies.

1. **Federal Supply Class:** 7195
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. **Horizontal:** Maximum 36 inches long / wide, 4 inches deep when closed, 23 inches high.
		2. **Vertical:** Maximum 22 inches long / wide, 6 inches deep when closed, 36 inches high.
	2. **Salient Characteristics that shall be provided:**
		1. Constructed of high-density polyethylene.
		2. Antimicrobial treatment / protection.
		3. Child protection straps and diaper bag holder.
		4. Built-in liner dispensers.
		5. Graphics and safety messages in at least four languages**.**

# Industry Standards / Requirement(s):

* + 1. **Industry Standards:** ASTM F2285 Standard Safety Performance Specification for Diaper Changing Tables.
		2. Warranty period shall be for 1 year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): Neutral.

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to mount and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (ea.) Horizontal \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (ea.) Vertical**

** **