1. **Purpose of this Equipment:** To transport and display fish products during special road show sales.
2. **Federal Supply Class:** 7310
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. 48 inches long / wide, 40 inches deep, 30 inches high. Dimensional sizes, such as length, width, and height are not critical to this equipment so long as this equipment is an upright floor model. They serve as a general guide to keep this equipment sized for available space.
	2. **Salient Characteristics that shall be provided:**
		1. Insulated
		2. Drain valve
		3. Stackable
		4. Movable by forklift or pallet jack
		5. Ice tray insert
		6. Lid for transporting
		7. Sneeze guard

# Industry Standards / Requirement(s):

* + 1. Industry Standards:Food and Drug Administration (FDA) approved materials.
		2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** N/A.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****