# Purpose of this Equipment: To allow patrons the opportunity to estimate the weight of their loose produce before final check out.

1. **Federal Supply Class:** 6670
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Scale face: 13 to 16 inch diameter.
		2. Commodity pan: 12 to 18 inch diameter, 3 to 5 inches deep.
	2. **Salient Characteristics that shall be provided:**
		1. Hanging scale:
			1. Chrome plated steel or stainless steel construction.
			2. Scale face enclosed.
			3. 30 lb. / 15kg capacity.
			4. Weight displayed in 1 ounce increments.
			5. Dampener system to reduce pointer oscillations.
			6. Hanging eye attached to top and bottom of scale housing.
			7. Scale face has large easy-to-read numbers.
		2. Commodity pan:
			1. Stainless steel.
			2. Removable.
			3. Steel support bracket for scale attachment.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
		2. Meets or exceeds weights and measures H-44, Class III requirements.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble, mount and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

