# Purpose of this Equipment: To hold the 2P05-A hanging scale at a comfortable height for commissary patrons.

1. **Federal Supply Class:** 6670
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 21 inches long / wide, 77 inches high (product within +/- 3 inches of the stated measurements will be deemed acceptable).
      2. Base to be circular with a diameter of 17 inches (product within +/- 1 inch of the stated measurements will be deemed acceptable).
      3. The bag must be no higher than 30 inches from the floor.
   2. **Salient Characteristics that shall be provided:**
      1. Steel construction.
      2. Cathedral shaped.
      3. Free standing.
      4. Powder coated, baked enamel.
      5. One plastic bag holder on each side of the stand.
      6. Minimum 25 pound base for stability.
      7. Hook for hanging scale.
      8. ADA compliant.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Black

1. **Electrical Requirements:**

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble and use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

