# Purpose of this Equipment: To store and move product in refrigerated and freezer areas.

1. **Federal Supply Class:** 7125
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 48 inches long, 24 inches wide, 69 inches high. Dimensions may vary 3 inches.
   2. **Salient Characteristics that shall be provided:**
      1. Minimum capacity of 900 lbs. per unit.
      2. Minimum 5 inch corrosion resistant, non-marking wheels.
      3. 4 swivel casters, minimum 2 locking.
      4. Stainless steel frame.
      5. Adjustable wire shelves.
      6. DonutBumpers.

# Industry Standards / Requirement(s):

* + 1. Industry Standards**:** National Sanitation Foundation (NSF) certification, or approved equivalent.
    2. Warranty period shall be for (1) year from date of delivery against defectivematerial and workmanship and shall include parts, service and labor.
  1. **Information Technology Requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble and use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****