# Purpose of this Equipment: To spot merchandise floral display.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 48 inches long / wide, 37 inches deep, 79 inches high.
      2. Dimensional sizes may vary plus or minus 2 inches in any direction.
   2. **Salient Characteristics that shall be provided:**
      1. Grid style top for hanging flower baskets.
      2. Construction: ABS, PVC, laminate or equivalent material.
      3. Casters: 2 swivels and 2 locking.
      4. Steps:
         1. Steps to be 48 inches long / wide, 13 inched deep.
         2. Each step to have ½ inch tall raised lip.
         3. First step to be 12 inches from floor.
         4. 10 inches rise between steps.
         5. All step measurements may vary plus or minus 2 inches in any direction.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Black

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped pre-drilled and ready to assemble.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****