# Purpose of this Equipment: To serve as end caps for produce displays and increase usable merchandising area.

1. **Federal Supply Class:** 7125
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. 2P30-S3R 36 inches long / wide, 12 inches deep, 50 inches high.
		2. 2P30-S3L 36 inches long / wide, 12 inches deep, 50 inches high.
		3. Dimensional sizes may vary plus or minus 3 inches in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Oak construction.
		2. Moisture resistant protective sealant.
		3. Casters: 2 swivel and minimum 2 locking per end cap.
		4. Creating a stacked crate effect.
		5. Bottom of crate merchandising area to be one solid piece of wood.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): Light Oak

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped pre-drilled and ready to assemble.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY:** \_\_\_\_\_ (ea) 2P30-S3R \_\_\_\_\_ (ea) 2P30-S3L

****