# Purpose of this Equipment: To hold pre-cooked or pre-warmed foods within a proper temperature range prior to serving. This unit is not designed to cook foods.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Dimensional sizes not to exceed 26 inches long / wide, 38 inches deep, 77 inches high.
   2. **Salient Characteristics that shall be provided:**
      1. Stainless steel exterior and interior.
      2. Thermostat heat control – must be able to maintain temperatures between 90 and 210 degrees Fahrenheit.
      3. Adjustable humidity.
      4. Right or left hinged door capability.
      5. Four casters, two locking.
      6. Accommodates a minimum of (12) ea. - 18 x 26 inch pans.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: Underwriters Laboratory (UL) listed and National Sanitation Foundation (NSF) certification, or approved equivalent.
    2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# Standard U.S.A. electrical specifications: 120 volts, 60 Hertz, 1 phase.

# \_\_\_\_\_ Pacific Theater stores 120 V / 50 HZ / 1 PH (Applies to these stores only: Atsugi, Misawa, Sagami, Sagamihara, Yokosuka, Yokota, Camp Zama, and Kanto Plains CDC. All other stores are standard U.S.A. 60 cycle voltages.)

# Minimum 6 foot cord with a NEMA Standard plug, or a manufacturer’s equivalent to comply with the equipment plug in requirements.

# NOTE: the operating range for 120 volts is 110 to 120 volts; the operating range for 220 volts is 208 to 230 volts.

# Standard Contractor Requirements:

* 1. Must be shipped ready to plug in,and use
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

**\_\_\_\_\_** Right hand hinged

**\_\_\_\_\_** Left hand hinged

****