1. **Purpose of this Equipment:** To transport and for temporary storage of meat products.
2. **Federal Supply Class:** 7320
3. **General Operating Specifications:**
   1. **Dimensions:**

**3.1.1** 2M03-A: 27 inches long / wide, 19 inches deep, 71 inches high.

**3.1.2** 2M03-B: 25 inches long / wide, 16 inches deep, 33 inches high.

**3.1.3** Dimensional sizes may vary no more than 1 inch in any direction.

* 1. **Salient Characteristics that shall be provided:**
     1. All welded stainless-steel frame with no nuts and bolts to loosen.
     2. Four heavy duty polyurethane swivel casters.
     3. Minimum of four inches in diameter casters.
     4. 6 Lugs (2M03-A) or 2 Lugs (2M03-B)

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Contractor Requirements:

* 1. Must be shipped ready to use
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY AND TYPE:**

**2M03-A \_\_\_\_\_\_\_\_\_\_\_** ( 6 lug) **2M03-B \_\_\_\_\_\_\_\_\_\_\_\_** (2 lug)

****