# Purpose of this Equipment: To transport and / or for temporary storage of meat products.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 36 inches long, 20 inches wide, 33 inches high.
      2. Dimensional sizes may vary no more than 1 inch in any direction.
   2. **Salient Characteristics that shall be provided:**
      1. Minimum load capacity of 500 pounds.
      2. Solid bottom platform to serve as drip pan
      3. Removable wire basket.
      4. Two each 5-inch non-marking front swivel casters; two each 8 inch non-marking rear wheels
      5. Constructed of nickel chrome finished tubular steel.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: National Sanitation Foundation (NSF) certification, or approved equivalent.
    2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology Requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****