# Purpose of this Equipment: To guide patrons into a queue for smooth check-out operations or restrict access to areas.

1. **Federal Supply Class:** 9905
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Poles: To be between 37 and 40 inches high. Not to exceed 3.5 inches diameter.
		2. Belts: Not to exceed 10 feet long, and 3 inches wide.
		3. Signs: Not to exceed vertical 7 inches wide x 11 inches high or horizontal 11 inches wide x 7 inches high.
		4. Base: Not to exceed 15 inch diameter.
	2. **Salient Characteristics that shall be provided:**
		1. Queuing system
			1. 4 way connection.
			2. Retractable belt.
			3. Non-marking base.
			4. Posts to be made of steel or aluminum.
			5. Base to be made of steel, or cast iron.
		2. Signs
			1. Black background with minimum 1 inch high white letters.
			2. Plastic or metal housing.
			3. Each sign includes a removable, adjustable sign adaptor / holder to firmly hold the sign at the top of the stanchion post.

# Industry Standards / Requirement(s): N / A

* 1. **Information Technology requirements**: N / A

# Color Requirement(s):

* + 1. Post and base: Chrome, stainless steel or black.

# Sign holder: Chrome, stainless steel or black

# Post and base: Chrome, stainless steel or black.

# Belt: Black

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assembleand use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

**Sign options.**

**\_\_\_\_\_ (ea) “PLEASE ENTER HERE” doubled faced signs.**

 **\_\_\_\_\_ (ea) “PLEASE WAIT HERE FOR NEXT AVAILABLE CASHIER” single faced signs.**

****