# Purpose of this Equipment: To vacuum wet or dry areas.

1. **Federal Supply Class:** 7910
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. N / A
	2. **Salient Characteristics that shall be provided:**
		1. Minimum 1.5 horsepower.
		2. Minimum 12-gallon tank.
		3. Dolly cart or wheeled for easy transport.
		4. Washable filters.
		5. Hose minimum 7 ft. in length and 1.5 inches in diameter.

# Industry Standards / Requirement(s):

* + 1. **Industry Standards*:*** Underwriters Laboratory (UL) listed or approved equivalent. Conformité Européene (CE) is not acceptable for a standard.
		2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# \_\_\_\_\_ Standard U.S.A. electrical specifications: 120 volts, 60 Hertz, 1 phase.

# Minimum 15-foot cord with a NEMA Standard plug, or a manufacturer’s equivalent to comply with the equipment plug in requirements.

# NOTE: the operating range for 120 volts is 110 to 120 volts; the operating range for 220 volts is 208 to 230 volts.

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble, plug in,and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****