# Purpose of this Equipment: To precisely portion ground meat into loaves for sales floor display

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. N / A
   2. **Salient Characteristics that shall be provided:**
      1. Height adjustable stand
      2. Attaches to and operates in tandem with main mixer / grinder unit (CED 1M20)
      3. Automatic paper feed unit inserts a paper separator between each square or molded meat block
      4. Portions 8 to 32 ounce loaves of ground meat
      5. Power unit, conveyor, knife and guide, extrusion die and adapter removable for cleansing
      6. Safety interlock switch disengages motor when power unit is removed
      7. Molder / bulker connects to mixer / grinder by means of adapter
      8. Shall accommodate size 32, size 42, or size 52 adapter to operate in tandem with various mixer / grinder manufacturers

# Industry Standards / Requirement(s):

* + 1. Industry Standards: Underwriters Laboratory (UL) listed and National Sanitation Foundation (NSF) certification, or approved equivalent. Conformité Européene (CE) is not acceptable for a standard.
    2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# \_\_\_\_\_ Standard U.S.A. electrical specifications: 115 volts, 60 Hertz, 1 phase.

# \_\_\_\_\_ Pacific Theater stores 120 / 220 V / 50 HZ / 1 PH (Applies to these stores only: Atsugi, Misawa, Sagami, Sagamihara, Yokosuka, Yokota, Camp Zama, and Kanto Plains CDC. All other stores are standard U.S.A. 60 cycle voltages.).

# Minimum 6-foot cord with a NEMA Standard plug, or a manufacturer’s equivalent to comply with the equipment plug in requirements.

# NOTE: the operating range for 120 volts is 110 to 120 volts; the operating range for 220 volts is 208 to 230 volts.

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble, plug in,and use
  2. This equipment requires disposal: place in a specified area
  3. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  4. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

1. **OTHER EQUIPMENT OPTIONS:**

**\_\_\_\_\_ Size 32 adapter**

**\_\_\_\_\_ Size 42 adapter**

**\_\_\_\_\_ Size 52 adapter**

****