# Purpose of this Equipment: To provide a comfortable chair that offers ergonomic features.

1. **Federal Supply Class:**  7110
2. **General Operating Specifications:**
   1. **Dimensions:**
      1. High-back dimensions (2A14-A): overall height 41 inches to 49 inches, seat height 17 inches to 23 inches, seat size, 17 inches wide by 17 to 23 inches deep, back size 19 inches wide by 18 inches to 28 inches high
      2. Low-back dimensions (2A14-B): overall height 34 inches to 42 inches, seat height 17 inches to 23 inches, seat size, 23 inches wide by 20 to 23 inches deep, back size 21 inches wide by 18 inches to 21inches high
   2. **Salient Characteristics that shall be provided:**
      1. Adjustable arms
      2. Swivel tilt/forward tilt mechanism
      3. Infinite position tilt-lock adjustment
      4. Memory foam cushion seat
      5. Pneumatic height adjustment with adjustable tension control
      6. Weight capacity 300 lbs
      7. Carpet casters

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Black

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble,and use
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_ (**each) 2A14-A (high back) **\_**\_\_\_ (each) A14-B (mid back)

 