1. **Purpose of this Equipment:** To provide transportation and storage of sheet pans
2. **Federal Supply Class:** 7125
3. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 21 inches long / wide, 27 inches deep, 33 inches high. Dimensional sizes, such as length, width, and height serve as a general guide to keep this equipment sized for available space.
   2. **Salient Characteristics that shall be provided:**
      1. Aluminum Framework 2 inch x 2inch x .125inch wall angle.
      2. Aluminum Handles and sides 1” x 1” x .070 wall tubing.
      3. Four 5” platform type swivel casters.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: National Sanitation Foundation (NSF) certification.
    2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to and use
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****