1. **Purpose of this Equipment:** To scan pictures and logos to create edible personalized cake decorations for the patrons.
2. **Federal Supply Class:** 7320
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. Minimum 15” monitor with standard keyboard and mouse or a touchscreen monitor.
	2. **Salient Characteristics that shall be provided:**

# Printer:

* + - 1. Copy, print and scan
			2. Printer to be top/gravity fed
			3. Minimum 5760 x 1440 print resolution (DPI)
			4. Minimum 9600 x 9600 scanning resolution (DPI)
			5. Capable of using FDA Approved 1/4 inch – 8.5 x 11 inch edible frosting sheets
			6. Capable of using FDA Approved edible ink cartridges or refillable ink set
		1. Computer:
			1. Keyboard of touch screen
			2. Mouse
			3. Monitor
			4. Ports and slots for CD/DVD, USB flash drive 2.0, and SD/MicroSD card’s
			5. Documentation CD-ROM with design software and drivers

# Industry Standards / Requirement(s):

* + 1. **Industry Standards:** Underwriters Laboratory (UL) listed. Conformité Européene (CE) is not acceptable for a standard.
		2. Ability to use FDA approved edible ink and frosting sheets.
		3. Warranty period shall be for a minimum 60 days from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# Standard U.S.A. electrical specifications: 120 volts, 60 Hertz, 1 phase.

# Minimum 5 foot cord with a NEMA Standard plug or a manufacturer’s equivalent to comply with the equipment plug in requirements.

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble, plug inand use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

