# Purpose of this Equipment: To provide a 360 degree bakery goods display for patron self-service selections.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. 49 inches long / wide, 54 inches deep, 45 inches high. (Double-sided table).
		2. 47 inches long / wide, 17 inches deep. (Bottom side shelf)
		3. 27 inches long / wide, 13 inches deep. (Top side shelf)
		4. Dimensional sizes may vary plus or minus 2 inches in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Consists of two separate sections, the double-sided table and two tier removable side shelves.
		2. Oak construction.
		3. Moisture resistant protective sealant.
		4. Casters, 2 swivel and minimum 2 locking.
		5. Four steel legs.
		6. Double sided table components:
			1. Bed-type top shelf that lies flat. (46 inches long / wide, 25 inches deep, 2 to 5 inches high)
			2. Pull-out drawer on each side that extends out 13 to 19 inches.
			3. Black plastic or flexible vinyl bumper on both pull-out drawers.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): Light Oak

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped assembled and ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****