# Purpose of this Equipment: To transport and merchandize cartons of eggs from the walk-in cooler side for patron’s selection.

1. **Federal Supply Class:** 7125
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 2G08-A: 38 inches long / wide 25 inches deep 66 inches high
      2. 2G08-B: 26 inches long / wide 25 inches deep 66 inches high
      3. Dimensional sizes, such as length, width, and height are allowed to vary + / - 2 inch

* 1. **Salient Characteristics that shall be provided:**
     1. 2G08-A, 360 carton capacity
        1. Four swivel castors
     2. 2G08-B, 240 carton capacity
        1. Two swivel, two fixed castors
     3. Hinged base and two shelves
     4. Folding design
     5. Tubular steel frame with zinc electroplate with lacquer dip finish

# Industry Standards / Requirement(s): N / A

* 1. **Information Technology Requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* + 1. Must be shipped ready to assembleand use.
    2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
       1. Point of Contact for Service.
       2. N / A
       3. N / A
    3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

2G08-A **\_\_\_\_\_\_\_\_\_\_\_\_\_** (360 dozen) 2G08-B\_\_\_\_\_\_\_\_\_\_\_ (240 dozen)

[](https://www.commissaries.com/aced/display_aced_image.cfm?ID=287)