# Purpose of this Equipment: To display and merchandise a variety of produce products.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Designed as a display cart 38 inches high with retractable and slatted steps that can expand from 40 inches (closed) to 80 inches (expanded).
		2. Dimensional sizes may vary plus or minus 2 inches in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Oak construction.
		2. Moisture-resistant protective sealant.
		3. Casters: 2 swivel and 2 locking.
		4. Three of the six slatted steps are retractable.
		5. Multi-use oak produce display cart with six steps for display.
		6. Supported by two rear 32 inch wooded wheels with rubber tires.
		7. Two legs each on the first and third expanded steps.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): Light Oak

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped pre-drilled and ready to assemble.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****