# Purpose of this Equipment: To accommodate 18 inch platters or pans for moving product.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. 26 inches long / wide, 21 inches deep, 70 inches high. Dimensional sizes may vary no more than 3 inches in any direction. The runners must be able to hold 18 inch wide platters or pans.
	2. **Salient Characteristics that shall be provided:**
		1. All Stainless steel construction.
		2. 1 ½ inch angle runners with six inch spacing.
		3. Accommodate 10 platters or pans.
		4. All four wheels to be swivel casters.
		5. 5 inches in diameter, polyurethane wheels.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: National Sanitation Foundation (NSF) certification, or approved equivalent. Conformité Européene (CE) is not acceptable for a standard.
		2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****