# Purpose of this Equipment: To provide commissary patrons a comfortable place to sit in a designated area.

1. **Federal Supply Class:** 7110
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. 48 inches wide, 25 inches deep, 30 inches high, (1E16-4)
		2. 72 inches wide, 25 inches deep, 30 inches high, (1E16-6)
		3. Dimensional sizes, such as length, width, depth and height should not vary by more than 3 inches in any dimension.
	2. **Salient Characteristics that shall be provided:**
		1. To be constructed of 100 percent commingled, post-consumer and / or post-industrial recycled plastic
		2. Free standing
		3. Without arms
		4. Supports (legs):

1E16-4: minimum 2 supports (legs)

1E16-6: minimum 3 supports (legs)

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): Brown with supports (legs) being black

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble and use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**1E16-4 QTY \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 1E16-6 QTY \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

****