# Purpose of this Equipment: To provide a staging area for recovering carts from the parking lot and help minimize damage to vehicles.

1. **Federal Supply Class:** 7290
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Units must fit inside one or two standard parking spaces (in line approximately 9ft wide by 19ft long) depending on the model selected for a specific application.
	2. **Salient Characteristics that shall be provided:**
		1. Galvanized cart rails
		2. Capable of being permanently mounted if required
		3. Bumper guards to protect car doors
		4. High generic signage or graphic indicating cart recovery location
		5. Single corral (2E11-A)
			1. Minimum 20 cart capacity (20,000 cubic inch model)
		6. Bi-directional corral (2E11-B)
			1. Minimum 40 cart capacity (20,000 cubic inch model)
			2. All parts included for bi-directional motorized cart retrieval, to include center separator bar and lane end chains.
		7. Covered corral (2E11-C)
			1. Minimum 30 cart capacity (20,000 cubic inch model)
			2. Peaked or Rounded Roof

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology Requirements:** N / A

# Color Requirement(s): Blue

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble with common tools and unskilled labor.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: As required. Approval from Area Operations is required.

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

 **2E11-A\_\_\_\_\_\_ 2E11-B\_\_\_\_\_\_\_ 2E11-C\_\_\_\_\_\_**

 ****

2E11-A

 2E11-B

 ****

 2E11-C