# Purpose of this Equipment: To transport merchandise for stocking shelves.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. 37 inches long, 18 inches wide, 41 inches high.
		2. Dimensional sizes may vary no more than 1 inch in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. All welded, steel tube construction.
		2. Minimum 750 pounds capacity.
		3. Two rigid and two swivel non-marking casters.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology Requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****