1. **Purpose of this Equipment:** To store important documents.
2. **Federal Supply Class:** 7110
3. **General Operating Specifications:**
   1. **Dimensions:** 
      1. **2A21-2:** 36 long / wide, 18 inches deep, and 28 inches high.
      2. **2A21-5:** 36 long / wide, 18 inches deep, and 65 inches high.

Dimensional sizes may vary by 2 inches in any direction.

* 1. **Salient Characteristics that shall be provided:**
     1. Recessed handles on drawers.
     2. Welded steel construction.
     3. Adjustable leveling glides.
     4. Powder coated or baked enamel finish.
     5. Ball bearing drawer track / slides.
     6. Drawer inter-lock system which allows for only one drawer to be open at a time.
     7. Locking system that secures all drawers.

# Industry Standards / Requirement(s):

* + 1. **Industry Standards**: American National Standards Institute / Business and Institutional Furniture Manufacture’s Association (ANSI/BIFMA) or approved equivalent**.**
    2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology Requirements:** N / A

# Color Requirement(s): Beige or gray.

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped assembled and ready to use*.*

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_\_ (ea.) 2A21-2 (2 drawer) \_\_\_\_\_\_\_\_ (ea.) 2A21-5 (5 drawer)**

****