# Purpose of this Equipment: For break room or cafeteria use consisting of table and four chairs.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Table:
			1. Top sizes to be 42 inches in diameter at a height of 29 inches above the floor.
		2. Chair:
			1. Overall dimensions to be 16 inches wide, 18 inches deep, 31 inches high. Dimensional sizes such as length, width, and height may vary up to 2 inches.
	2. **Salient Characteristics that shall be provided:**
		1. Table:
			1. Square table top constructed of non-marring or high pressure laminate on a minimum of a 1inch core top.
			2. Base to be cast iron or tubular steel in an x-frame design with four feet.
			3. T-mold edge band or banding.
			4. Powder coated or chrome finish base.
		2. Chair:
			1. Polypropylene or vinyl seat.
			2. Minimum 300 pound weight capacity.
			3. One carton per table (4 chairs).

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s):

# Laminate table top finish: Dark wood grain (mahogany or walnut).

* + 1. **Frame for table base and chairs:** Black or chrome.
		2. **Chair finish:** Black or burgundy.
1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****