# Purpose of this Equipment: For break room or cafeteria use consisting of table and four chairs.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Table:
         1. Top sizes to be 42 inches in diameter at a height of 29 inches above the floor.
      2. Chair:
         1. Overall dimensions to be 16 inches wide, 18 inches deep, 31 inches high. Dimensional sizes such as length, width, and height may vary up to 2 inches.
   2. **Salient Characteristics that shall be provided:**
      1. Table:
         1. Square table top constructed of non-marring or high pressure laminate on a minimum of a 1inch core top.
         2. Base to be cast iron or tubular steel in an x-frame design with four feet.
         3. T-mold edge band or banding.
         4. Powder coated or chrome finish base.
      2. Chair:
         1. Polypropylene or vinyl seat.
         2. Minimum 300 pound weight capacity.
         3. One carton per table (4 chairs).

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s):

# Laminate table top finish: Dark wood grain (mahogany or walnut).

* + 1. **Frame for table base and chairs:** Black or chrome.
    2. **Chair finish:** Black or burgundy.

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble and use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****